Harsiddh Profile

Established in 1987 **HARSIDDH PHARMAMACH PVT LTD** (formerly: **HARSIDDH INDUSTRIES**) has completed 35 years now. Backed up by long and vast experience in the line we manufacture complete aseptic packaging line solutions for liquid and injectable in sterile conditions with latest advanced technologies with innovative ideas to render satisfactory performance round-the-clock. The machines can work either individually or form a complete production line.

We offer a high level of innovation and development along with the flexibility to adapt each project to the specific needs of the customer.

HARSIDDH has on its client list number of renowned companies in India and abroad and meet with international norms being one of the rapidly growing exporters of pharmaceutical equipment. Our sales team, project management and after sales service operate at a global level to create HARSIDDH’s brand value in global market.

Product Details

1. Complete Injectable Liquid Vial Filling Line.
2. Complete Injectable Dry Powder Vial Filling Line.
3. Complete Ampoule Filling Line.
4. Complete MDI Line
5. Complete Nasal Line
6. Complete Bottle Line
7. Complete Ophthalmic (Eyedrops) Line
8. Semi-Automatic IV Bag filling Machine with inline CIP & SIP
9. Automatic PFS Filling and Stoppering Line
10. Automatic Linear Vial Washing Machine
11. Automatic Rotary Vial/Ampoule Washing Machine
12. Automatic Air Jet Cleaning Machine for Jar/Bottle
13. Automatic Bottle Unscrambler
14. Automatic Bottle Washing Machine
15. Automatic Vial/Ampoule External Washing Machine
16. Automatic Vial Filling & Stoppering Machine
17. Automatic Bottle Filling Machine
18. Automatic Vial/Bottle Capping Machine
19. Automatic Label Counter
20. Automatic Self-Adhesive Sticker Labelling Machine for Ampoule, Vial & Bottle
21. Automatic Tablet/Capsule Elevator
22. Automatic Leaflet Pasting Machine
23. Automatic Vertical Ampoule Filling & Sealing Machine
24. Semi-Automatic Rotary Cartoning Machine
25. Fully Automatic Cartoning Machine
26. Automatic Two Stage Tray Loading Machine
27. Conveyors & Turn Table

AUTOMATIC ROTARY VIAL/AMPOULE WASHING MACHINE

|  |
| --- |
| **Ophthalmic Line**   1. **Automatic Bottle Unscrambler Machine with Bottle Feeder** 2. **Automatic Monoblock Liquid Filling, Insert Plugging & Screw Capping Machine** |
| **Automatic Rotary Type Nasal Line for Round bottle**   1. **Automatic Bottle Unscrambler Machine with Bottle Feeder** 2. **Automatic Monoblock Liquid Filling, Pump Placement, Crimping and Actuator Placement Machine** |
| **Automatic Rotary Type Nasal Line for Oval Shaped/Round bottle**   1. **Automatic Bottle Unscrambler Machine with Bottle Feeder** 2. **Automatic Bottle Airjet Cleaning Machine** 3. **Automatic Continuous Motion Bottle Filling, Plug Placing and Pressing with Screw Capping Machine** |
| **Automatic Linear Type Nasal Line for Round bottle**   1. **Automatic Bottle Unscrambler Machine with Bottle Feeder** 2. **Automatic Liquid Filling, Pump Placement and Crimping Machine** 3. **Automatic Actuator Placement and Dust Cap Placement Machine** |
| **Automatic Metered Dose Inhalers Filling (MDI Lines)**   1. **Automatic Can Unscrambler Machine with Can Feeder** 2. **Automatic Can Cleaning Machine** 3. **Automatic Aerosol Can Filling and Crimping Machine with Pump Placement Unit** 4. **Automatic Water stress Bath Machine** 5. **Automatic Two Stage Tray Loader Machine.** |

New Image

|  |  |
| --- | --- |
| **AUTOMATIC TWO STAGE TRAY LOADING COLLECTION**  **Silent Features:**   * To supply Tray loader to automatically load bottles into trays. * Machine has possibilities to incorporate single or two tray. * The loading devices with nesting pistons to load rows of cans into alternate 3sided trays * Integral electrical panel with PLC control system * Change parts for one tray type and one Bottle diameter. * Can Loading with Zig Zag Mechanism * Single Pusher arrangement with dual tray system | **Automatic Two Stage Tray Loading Machine** |
| **AUTOMATIC INVERTER AIR JET CLEANING MACHINE FOR BOTTLES AND JARS**  **Silent Features:**   * Cleaning with help of pressurized air through needle and (Optional)   ionized air   * Suitable for 10ml to 250ml containers (with the help of change parts) * Complete cGMP model. * All contact parts with the internal surface of Container and the wash media are made from AISI 316L Stainless Steel. * Non-contact parts are made from engineering plastic, AISI SS 304 or other FDA approved material. * All finishes, welding joints are processed, treated & equipment selected in accordance with cGMP standards. * Machine is equipped with PLC system with passwords. | **Automatic Inverter type Airjet Cleaning Machine for bottle** |
| **AUTOMATIC UNSCRAMBLER MACHINE WITH BOTTLE FEEDER**  **Silent Features:**   * Stainless steel frame with stainless steel cladding * Integral bottle hopper with level indication. * Integral elevator with movement control * Horizontal rotating selector disc with level control * Adjustable air jets to aid sorting process * Air-Jet Cleaning Station with Air Ionizer (Optional) * Transfer conveyor to bottle orientation unit with queue control. * The unit is totally covered with safety cabinet Features: | **Automatic Bottle Unscrambler Machine with Bottle Feeder** |